IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView_V2.0]"
Description: "ExchangeRequirement []"
Time stamp: "2022-09-12T16:09:48"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "22.0.2.392 - Exporter 22.0.2.392 - Default UI"
Application: "Autodesk Revit 2022 (ENU)" version "2022" identifier "Revit" by Organization "Autodesk Revit 2022 (ENU)"

People and organizations
  Person "dev2NW3Q" of Organization (no name given)
  Owner history of Person "dev2NW3Q" of Organization (no name given) | application "Autodesk Revit 2022 (ENU)" version "2022" identifier "Revit" by Organization "Autodesk Revit 2022 (ENU)" | change NOCHANGE | created 1662991787 (2022-09-12T14:09:47Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  MOMENTOFINERTIAUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"
  LINEARFORCEUNIT: derived
  PLANARFORCEUNIT: derived

Spatial structure
IFCPROJECT
  IFCSITE "Default" | latitude 42° 24′ 53.508911″ | longitude -71° 15′ 29.058837″ | elevation above sea level 0.
    IFCBUILDING | postal address (none given)
      IFCBUILDINGSTOREY "Level 1" | long name "Level 1" | object type "Level:Level 1" | elevation 0.
        contains 1 element
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "FR - 180 ATJ:180 ATJ" | object type "FR - 180 ATJ:180 ATJ" | names: "FR - 180 ATJ:180 ATJ:24339" | material: materials ("255_0_0", "26_26_26", "Acier Noir", "Par défaut") | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Dimensions

Types
  IFCBUILDINGELEMENTPROXYTYPE "FR - 180 ATJ:180 ATJ" | 1 occurrence | material: "255_0_0" | property sets: Constraints, Construction, Data, Dimensions, Energy Analysis, Green Building Properties

Property sets
  Pset_ProductRequirements | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY) | on 1 type object
    Category = "Specialty Equipment" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Name = "Level 1" (IFCLABEL)
  Other | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
  Other | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Category = "Specialty Equipment" (IFCLABEL)
    Family = "FR - 180 ATJ: 180 ATJ" (IFCLABEL)
    Family and Type = "FR - 180 ATJ: 180 ATJ" (IFCLABEL)
    Type = "FR - 180 ATJ: 180 ATJ" (IFCLABEL)
    Type Id = "FR - 180 ATJ: 180 ATJ" (IFCLABEL)
  Other | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family = "Level: Level 1" (IFCLABEL)
    Family and Type = "Level: Level 1" (IFCLABEL)
    Type = "Level: Level 1" (IFCLABEL)
    Type Id = "Level: Level 1" (IFCLABEL)
  Other | properties | on 1 type object
    Bruit à l'environnement (LwA) en dB(A) = 105. (IFCREAL)
    Category = "Specialty Equipment" (IFCLABEL)
    Consommation carburant (l/jour) = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Emissions de CO2 (g/kWh) = 3.4 (IFCREAL)
    Family Name = "FR - 180 ATJ" (IFCTEXT)
    MasterFormat = "Operation and Maintenance of Transportation" (IFCTEXT)
    Masterformat Code = "34 01 00" (IFCTEXT)
    Max Number of People = 2. (IFCREAL)
    Max Working Height = 18190. (IFCLENGTHMEASURE) [MILLI METRE]
    Maximum Load Supported (Fork or Pod) = 350. (IFCMASSMEASURE) [KILO GRAM]
    OmniClass code = "23-23 00 00" (IFCTEXT)
    OmniClass description = "Conveying Systems and Material Handling Products" (IFCTEXT)
    Rated motor power = 18500. (IFCPOWERMEASURE) [WATT]
    Turning Radius = 3750. (IFCLENGTHMEASURE) [MILLI METRE]
    Uniformat = "Other Conveying Systems" (IFCTEXT)
    Uniformat code = "D1090" (IFCTEXT)
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY) | on 1 type object
    Reference = "180 ATJ" (IFCIDENTIFIER)
  Pset_ManufacturerTypeInformation | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY) | on 1 type object
    Manufacturer = "MANITOU" (IFCLABEL)
  Pset_QuantityTakeOff | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY) | on 1 type object
    Reference = "180 ATJ" (IFCIDENTIFIER)
  Constraints | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Elevation from Level = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Host = "None" (IFCTEXT)
    Moves With Nearby Elements = FALSE (IFCBOOLEAN)
    Offset from Host = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    R2 = 45. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 type object
    Capacité de la nacelle = 230. (IFCMASSMEASURE) [KILO GRAM]
    Default Elevation = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Déport du contrepoids avec tourelle à 90° = 220. (IFCLENGTHMEASURE) [MILLI METRE]
    Déport max = 10510. (IFCLENGTHMEASURE) [MILLI METRE]
    Dévers autorisé = 5. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Hauteur de levage max = 18190. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Abaque Visible = TRUE (IFCBOOLEAN)
    Angle Pendulaire Souhaité = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Angle du Bras Télescopique Souhaité = 40. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Area = 41.3513985285346 (IFCAREAMEASURE) [SQUARE_METRE]
    Déport Réel = 7034.998000897 (IFCLENGTHMEASURE) [MILLI METRE]
    Hauteur Base du Bras téléscopique souhaitée = 4790. (IFCLENGTHMEASURE) [MILLI METRE]
    Hauteur Panier Réelle = 8684.93504080936 (IFCLENGTHMEASURE) [MILLI METRE]
    Longueur déploiement Bras Téléscopique = 1533. (IFCLENGTHMEASURE) [MILLI METRE]
    Rayon de Giration Visible = TRUE (IFCBOOLEAN)
    Rotation Panier = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Rotation Tourelle / Chassis = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Réglages du Pendulaire = TRUE (IFCBOOLEAN)
    Volume = 4.695489712935 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Computation Height = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 1 type object
    Floor Height = 400. (IFCLENGTHMEASURE) [MILLI METRE]
    Max Offset = 10510. (IFCLENGTHMEASURE) [MILLI METRE]
    Overall height = 2470. (IFCLENGTHMEASURE) [MILLI METRE]
    Overall length = 7790. (IFCLENGTHMEASURE) [MILLI METRE]
    Overall width = 2320. (IFCLENGTHMEASURE) [MILLI METRE]
  Electrical - Loads | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Circuit Number = "" (IFCTEXT)
    Panel = "" (IFCTEXT)
  Phasing | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Phase Created = "New Construction" (IFCLABEL)
  Pset_AirSideSystemInformation | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "Level 1" (IFCLABEL)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Building Story = TRUE (IFCBOOLEAN)
    Name = "Level 1" (IFCTEXT)
    Structural = FALSE (IFCBOOLEAN)
  Identity Data | properties | on 1 type object
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    BC_MODEL_ID = "760565" (IFCTEXT)
    BC_OBJECT_ID = "214627" (IFCTEXT)
    BC_OBJECT_VERSION = "#1" (IFCTEXT)
    BC_VARIANT_ID = "527050" (IFCTEXT)
    Code Name = "" (IFCTEXT)
    Créé par = "ATLANCAD" (IFCTEXT)
    GTIN (Global Trade Item Number) = "" (IFCTEXT)
    Manufacturer = "MANITOU" (IFCTEXT)
    Manufacturer Product Link = "https://www.manitou.com/fr-FR/nos-machines/nacelles-elevatrices/180-atj" (IFCTEXT)
    Model = "180 ATJ" (IFCTEXT)
    Object type = "" (IFCTEXT)
    OmniClass Number = "23.50.00.00" (IFCTEXT)
    OmniClass Title = "Conveying Systems & Material Handling" (IFCTEXT)
    Reference = "180 ATJ" (IFCTEXT)
    Type Comments = "Nacelle élévatrice Diesel de 18m de hauteur de travail" (IFCTEXT)
    Type Name = "180 ATJ" (IFCTEXT)
    URL = "www.manitou.com" (IFCTEXT)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    IsLandmarked = UNKNOWN (IFCLOGICAL)
    NumberOfStoreys = 1 (IFCINTEGER)
  Constraints(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation Base = "Project Base Point" (IFCIDENTIFIER)
  Graphics(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Color = 0 (IFCINTEGER)
    Line Pattern = "Solid" (IFCLABEL)
    Line Weight = "1" (IFCIDENTIFIER)
    Symbol at End 1 Default = FALSE (IFCBOOLEAN)
    Symbol at End 2 Default = TRUE (IFCBOOLEAN)
  Identity Data(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Type Name = "Level 1" (IFCTEXT)
  Other(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family Name = "Level" (IFCTEXT)
  Construction | properties | on 1 type object
    Consommation moyenne = 0.000355555555555555 (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Tank Capacity = 0.052 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Unloaded Weight = 7430. (IFCMASSMEASURE) [KILO GRAM]
  Data | properties | on 1 type object
    Empattement = 2200. (IFCLENGTHMEASURE) [MILLI METRE]
    Garde au sol = 400. (IFCLENGTHMEASURE) [MILLI METRE]
    Garde au sol au centre de l'empattement = 400. (IFCLENGTHMEASURE) [MILLI METRE]
    Hauteur hors tout repliée = 2560. (IFCLENGTHMEASURE) [MILLI METRE]
    Hauteur plancher = 400. (IFCLENGTHMEASURE) [MILLI METRE]
    Hauteur position transport = 2475. (IFCLENGTHMEASURE) [MILLI METRE]
    Largeur = 2320. (IFCLENGTHMEASURE) [MILLI METRE]
    Largeur du panier = 800. (IFCLENGTHMEASURE) [MILLI METRE]
    Longueur du panier = 1800. (IFCLENGTHMEASURE) [MILLI METRE]
    Longueur hors tout repliée = 5560. (IFCLENGTHMEASURE) [MILLI METRE]
    Longueur position transport = 7790. (IFCLENGTHMEASURE) [MILLI METRE]
    Masse à vide = 7470. (IFCMASSMEASURE) [KILO GRAM]
    Nombre de personne (Interieur Extérieur) = 2 (IFCINTEGER)
    Norme du moteur = "Directives Européennes : 2006/42/CE - Machines (refonte EN280-2013) - 2004/108/EC (EMC) - 2006/95/CE (Basse tension)" (IFCTEXT)
    Norme moteur = "Stage V" (IFCTEXT)
    Poids de la nacelle = 7430. (IFCMASSMEASURE) [KILO GRAM]
    Rayon de giration 4RD ext = 3750. (IFCLENGTHMEASURE) [MILLI METRE]
    Rayon de giration 4RD int = 1380. (IFCLENGTHMEASURE) [MILLI METRE]
    Surplomb = 7550. (IFCLENGTHMEASURE) [MILLI METRE]
    longueur pendulaire = 1700. (IFCLENGTHMEASURE) [MILLI METRE]
  Energy Analysis | properties | on 1 type object
    Consommation moyenne (L/h) = 1.281 (IFCREAL)
    Puissance du moteur I.C. (ch) = 24.8 (IFCREAL)
    Puissance du moteur I.C. (kW) = 18.5 (IFCREAL)
  Green Building Properties | properties | on 1 type object
    CO2 = 0. (IFCREAL)