IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView_V2.0]"
Description: "ExchangeRequirement []"
Time stamp: "2022-09-12T16:04:52"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "22.0.2.392 - Exporter 22.0.2.392 - Default UI"
Application: "Autodesk Revit 2022 (ENU)" version "2022" identifier "Revit" by Organization "Autodesk Revit 2022 (ENU)"

People and organizations
  Person "dev2NW3Q" of Organization (no name given)
  Owner history of Person "dev2NW3Q" of Organization (no name given) | application "Autodesk Revit 2022 (ENU)" version "2022" identifier "Revit" by Organization "Autodesk Revit 2022 (ENU)" | change NOCHANGE | created 1662991491 (2022-09-12T14:04:51Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  MOMENTOFINERTIAUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"
  LINEARFORCEUNIT: derived
  PLANARFORCEUNIT: derived

Spatial structure
IFCPROJECT
  IFCSITE "Default" | latitude 42° 24′ 53.508911″ | longitude -71° 15′ 29.058837″ | elevation above sea level 0.
    IFCBUILDING | postal address (none given)
      IFCBUILDINGSTOREY "Level 1" | long name "Level 1" | object type "Level:Level 1" | elevation 0.
        contains 1 element
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "EN - 100 VJR:100 VJR" | object type "EN - 100 VJR:100 VJR" | names: "EN - 100 VJR:100 VJR:13750" | material: materials ("Par défaut", "60_60_60", "Roues_100VJR_255_250_240", "Roues_191 191 191", "Tolerie_60_60_60", "Carrosserie 255_0_0", "Rouge Manitou", "Acier Noir", "<Unnamed>") | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ProvisionForVoid, Constraints

Types
  IFCBUILDINGELEMENTPROXYTYPE "EN - 100 VJR:100 VJR" | 1 occurrence | material: "Par défaut" | property sets: Constraints, Construction, Data, Dimensions, Energy Analysis, Green Building Properties

Property sets
  Pset_ProductRequirements | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY) | on 1 type object
    Category = "Specialty Equipment" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Name = "Level 1" (IFCLABEL)
  Other | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
  Other | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Category = "Specialty Equipment" (IFCLABEL)
    Family = "EN - 100 VJR: 100 VJR" (IFCLABEL)
    Family and Type = "EN - 100 VJR: 100 VJR" (IFCLABEL)
    Type = "EN - 100 VJR: 100 VJR" (IFCLABEL)
    Type Id = "EN - 100 VJR: 100 VJR" (IFCLABEL)
  Other | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family = "Level: Level 1" (IFCLABEL)
    Family and Type = "Level: Level 1" (IFCLABEL)
    Type = "Level: Level 1" (IFCLABEL)
    Type Id = "Level: Level 1" (IFCLABEL)
  Other | properties | on 1 type object
    Average consumption (l/day) = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    CO2 emissions (g/kWh) = 0. (IFCREAL)
    Category = "Specialty Equipment" (IFCLABEL)
    Family Name = "EN - 100 VJR" (IFCTEXT)
    MasterFormat = "Operation and Maintenance of Transportation" (IFCTEXT)
    Masterformat Code = "34 01 00" (IFCTEXT)
    Max Number of People = 2. (IFCREAL)
    Max Working Height = 9850. (IFCLENGTHMEASURE) [MILLI METRE]
    Maximum Load Supported (Fork or Pod) = 200. (IFCMASSMEASURE) [KILO GRAM]
    Noise to environment (LwA) = 0. (IFCREAL)
    OmniClass code = "23-23 00 00" (IFCTEXT)
    OmniClass description = "Conveying Systems and Material Handling Products" (IFCTEXT)
    Rated motor power = 1500. (IFCPOWERMEASURE) [WATT]
    Turning Radius = 2090. (IFCLENGTHMEASURE) [MILLI METRE]
    Uniformat = "Autres systèmes transporteurs" (IFCTEXT)
    Uniformat code = "D1090" (IFCTEXT)
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY) | on 1 type object
    Reference = "100 VJR" (IFCIDENTIFIER)
  Pset_ManufacturerTypeInformation | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY) | on 1 type object
    Manufacturer = "MANITOU" (IFCLABEL)
  Pset_QuantityTakeOff | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY) | on 1 type object
    Reference = "100 VJR" (IFCIDENTIFIER)
  Pset_ProvisionForVoid | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY) | on 1 type object
    Width = 990. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Elevation from Level = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Host = "None" (IFCTEXT)
    Moves With Nearby Elements = FALSE (IFCBOOLEAN)
    Offset from Host = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    R2 = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 type object
    Counterweight offset (turret at 90°) = 90. (IFCLENGTHMEASURE) [MILLI METRE]
    Default Elevation = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Max. lifting height = 9850. (IFCLENGTHMEASURE) [MILLI METRE]
    Max. outreach = 3150. (IFCLENGTHMEASURE) [MILLI METRE]
    Permissible leveling = 2. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Platform capacity = 200. (IFCMASSMEASURE) [KILO GRAM]
  Dimensions | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Actual Platform height = 887.703468591236 (IFCLENGTHMEASURE) [MILLI METRE]
    Actual offset = 2018.41318938308 (IFCLENGTHMEASURE) [MILLI METRE]
    Area = 16.6308643523179 (IFCAREAMEASURE) [SQUARE_METRE]
    Desired Platform angle = -50. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Desired telescopic mast height = 2000. (IFCLENGTHMEASURE) [MILLI METRE]
    External turning radius (over tyres) = TRUE (IFCBOOLEAN)
    Jib adjustment = TRUE (IFCBOOLEAN)
    Turret rotation = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Visible Charts = TRUE (IFCBOOLEAN)
    Volume = 1.32945961835593 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Computation Height = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 1 type object
    Empattement = 1200. (IFCLENGTHMEASURE) [MILLI METRE]
    Floor Height = 510. (IFCLENGTHMEASURE) [MILLI METRE]
    Garde au sol = 90. (IFCLENGTHMEASURE) [MILLI METRE]
    Max Offset = 3150. (IFCLENGTHMEASURE) [MILLI METRE]
    Overall height = 1990. (IFCLENGTHMEASURE) [MILLI METRE]
    Overall length = 2800. (IFCLENGTHMEASURE) [MILLI METRE]
    Overall width = 990. (IFCLENGTHMEASURE) [MILLI METRE]
  Electrical - Loads | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Circuit Number = "" (IFCTEXT)
    Panel = "" (IFCTEXT)
  Phasing | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Phase Created = "New Construction" (IFCLABEL)
  Pset_AirSideSystemInformation | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "Level 1" (IFCLABEL)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Building Story = TRUE (IFCBOOLEAN)
    Name = "Level 1" (IFCTEXT)
    Structural = FALSE (IFCBOOLEAN)
  Identity Data | properties | on 1 type object
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    BC_MODEL_ID = "775847" (IFCTEXT)
    BC_OBJECT_ID = "213442" (IFCTEXT)
    BC_OBJECT_VERSION = "#1" (IFCTEXT)
    BC_VARIANT_ID = "522371" (IFCTEXT)
    Code Name = "" (IFCTEXT)
    Créé par = "ATLANCAD" (IFCTEXT)
    GTIN (Global Trade Item Number) = "" (IFCTEXT)
    Manufacturer = "MANITOU" (IFCTEXT)
    Manufacturer Product Link = "https://www.manitou.com/fr-FR/nos-machines/nacelles-elevatrices/100-vjr" (IFCTEXT)
    Model = "100 VJR" (IFCTEXT)
    Object type = "Electric articulated work platform" (IFCTEXT)
    OmniClass Number = "23.50.00.00" (IFCTEXT)
    OmniClass Title = "Conveying Systems & Material Handling" (IFCTEXT)
    Reference = "100 VJR" (IFCTEXT)
    Type Name = "100 VJR" (IFCTEXT)
    URL = "www.manitou.fr" (IFCTEXT)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    IsLandmarked = UNKNOWN (IFCLOGICAL)
    NumberOfStoreys = 1 (IFCINTEGER)
  Constraints(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation Base = "Project Base Point" (IFCIDENTIFIER)
  Graphics(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Color = 0 (IFCINTEGER)
    Line Pattern = "Solid" (IFCLABEL)
    Line Weight = "1" (IFCIDENTIFIER)
    Symbol at End 1 Default = FALSE (IFCBOOLEAN)
    Symbol at End 2 Default = TRUE (IFCBOOLEAN)
  Identity Data(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Type Name = "Level 1" (IFCTEXT)
  Other(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family Name = "Level" (IFCTEXT)
  Construction | properties | on 1 type object
    Consommation moyenne = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Puissance du moteur I.C. (kW) = 1.5 (IFCREAL)
    Unloaded Weight = 2650. (IFCMASSMEASURE) [KILO GRAM]
  Data | properties | on 1 type object
    Engine norm = "A préciser" (IFCTEXT)
    External turning radius = 2090. (IFCLENGTHMEASURE) [MILLI METRE]
    Floor height (access) = 510. (IFCLENGTHMEASURE) [MILLI METRE]
    Ground clearance = 20. (IFCLENGTHMEASURE) [MILLI METRE]
    Ground clearance at centre of wheelbase = 90. (IFCLENGTHMEASURE) [MILLI METRE]
    Internal turning radius (over tyres) = 590. (IFCLENGTHMEASURE) [MILLI METRE]
    Jib length = 1500. (IFCLENGTHMEASURE) [MILLI METRE]
    Norme du moteur = "Directives Européennes : 2006/42/CE - Machines (refonte EN280-2013) - 2004/108/EC (EMC) - 2006/95/CE (Basse tension)" (IFCTEXT)
    Number of people (inside) = 2 (IFCINTEGER)
    Number of people (outside) = 1 (IFCINTEGER)
    Overall height (stowed) = 1990. (IFCLENGTHMEASURE) [MILLI METRE]
    Overall height (transport) = 1995. (IFCLENGTHMEASURE) [MILLI METRE]
    Overall lenght (stowed) = 2800. (IFCLENGTHMEASURE) [MILLI METRE]
    Overall lenght (transport) = 2810. (IFCLENGTHMEASURE) [MILLI METRE]
    Overhang = 6670. (IFCLENGTHMEASURE) [MILLI METRE]
    Platform dimensions (length) = 1110. (IFCLENGTHMEASURE) [MILLI METRE]
    Platform dimensions (width) = 930. (IFCLENGTHMEASURE) [MILLI METRE]
    Platform weight = 2650. (IFCMASSMEASURE) [KILO GRAM]
    Wheelbase = 1200. (IFCLENGTHMEASURE) [MILLI METRE]
    Width = 990. (IFCLENGTHMEASURE) [MILLI METRE]
  Energy Analysis | properties | on 1 type object
    Average consumption (L/h) = 0. (IFCREAL)
    I.C. Engine power rating - Power (ch) = 0. (IFCREAL)
    I.C. Engine power rating - Power (kW) = 0. (IFCREAL)
  Green Building Properties | properties | on 1 type object
    CO2 = 0. (IFCREAL)