IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView_V2.0]"
Description: "ExchangeRequirement []"
Time stamp: "2022-09-12T16:15:10"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "22.0.2.392 - Exporter 22.0.2.392 - Default UI"
Application: "Autodesk Revit 2022 (ENU)" version "2022" identifier "Revit" by Organization "Autodesk Revit 2022 (ENU)"

People and organizations
  Person "dev2NW3Q" of Organization (no name given)
  Owner history of Person "dev2NW3Q" of Organization (no name given) | application "Autodesk Revit 2022 (ENU)" version "2022" identifier "Revit" by Organization "Autodesk Revit 2022 (ENU)" | change NOCHANGE | created 1662992109 (2022-09-12T14:15:09Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  MOMENTOFINERTIAUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"
  LINEARFORCEUNIT: derived
  PLANARFORCEUNIT: derived

Spatial structure
IFCPROJECT
  IFCSITE "Default" | latitude 42° 24′ 53.508911″ | longitude -71° 15′ 29.058837″ | elevation above sea level 0.
    IFCBUILDING | postal address (none given)
      IFCBUILDINGSTOREY "Level 1" | long name "Level 1" | object type "Level:Level 1" | elevation 0.
        contains 1 element
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "EN - MT 625:MT 625" | object type "EN - MT 625:MT 625" | names: "EN - MT 625:MT 625:12016" | material: materials ("1_BLANC", "26_26_26", "240_171_0", "255_0_0", "0_Acier", "1_ROUGE 2") | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Dimensions

Types
  IFCBUILDINGELEMENTPROXYTYPE "EN - MT 625:MT 625" | 1 occurrence | material: "1_BLANC" | property sets: Constraints, Construction, Data, Dimensions, Energy Analysis, Green Building Properties

Property sets
  Pset_ProductRequirements | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY) | on 1 type object
    Category = "Specialty Equipment" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Name = "Level 1" (IFCLABEL)
  Other | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
  Other | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Category = "Specialty Equipment" (IFCLABEL)
    Family = "EN - MT 625: MT 625" (IFCLABEL)
    Family and Type = "EN - MT 625: MT 625" (IFCLABEL)
    Type = "EN - MT 625: MT 625" (IFCLABEL)
    Type Id = "EN - MT 625: MT 625" (IFCLABEL)
  Other | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family = "Level: Level 1" (IFCLABEL)
    Family and Type = "Level: Level 1" (IFCLABEL)
    Type = "Level: Level 1" (IFCLABEL)
    Type Id = "Level: Level 1" (IFCLABEL)
  Other | properties | on 1 type object
    CO2 emissions = 9.62 (IFCREAL)
    Category = "Specialty Equipment" (IFCLABEL)
    Charge Maximum supportée (Fourche ou Nacelle) = 2500. (IFCMASSMEASURE) [KILO GRAM]
    Charge à Déport Max = 800. (IFCMASSMEASURE) [KILO GRAM]
    Charge à Hauteur Max = 2000. (IFCMASSMEASURE) [KILO GRAM]
    Code Masterformat = "34 01 00" (IFCTEXT)
    Code Uniformat = "D1090" (IFCTEXT)
    Description OmniClass = "Conveying Systems and Material Handling Products" (IFCTEXT)
    Family Name = "EN - MT 625" (IFCTEXT)
    MasterFormat = "Operation and Maintenance of Transportation" (IFCTEXT)
    Noise at driving position (LpA) in dB(A) = 76. (IFCREAL)
    Noise to environment (LwA) = 104. (IFCREAL)
    Numéro OmniClass = "23-23 00 00" (IFCTEXT)
    Rayon de Braquage = 3310. (IFCLENGTHMEASURE) [MILLI METRE]
    Uniformat = "Autres systèmes transporteurs" (IFCTEXT)
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Reference = "MT 625" (IFCIDENTIFIER)
  Pset_ManufacturerTypeInformation | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY) | on 1 type object
    Manufacturer = "MANITOU" (IFCLABEL)
  Pset_QuantityTakeOff | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Reference = "MT 625" (IFCIDENTIFIER)
  Constraints | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Elevation from Level = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Host = "None" (IFCTEXT)
    Moves With Nearby Elements = FALSE (IFCBOOLEAN)
    Offset from Host = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 type object
    Default Elevation = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Max. capacity = 2500. (IFCMASSMEASURE) [KILO GRAM]
    Max. lifting height = 5850. (IFCLENGTHMEASURE) [MILLI METRE]
    Max. outreach = 3400. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Area = 22.3824400835418 (IFCAREAMEASURE) [SQUARE_METRE]
    Desired lifting height = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Desired offset = 1219. (IFCLENGTHMEASURE) [MILLI METRE]
    External turning radius (over tyres) = TRUE (IFCBOOLEAN)
    Max offset = FALSE (IFCBOOLEAN)
    Visible Charts = TRUE (IFCBOOLEAN)
    Volume = 3.61330135991962 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Computation Height = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 1 type object
    Déport Max = 3400. (IFCLENGTHMEASURE) [MILLI METRE]
    Empattement = 2300. (IFCLENGTHMEASURE) [MILLI METRE]
    Garde au sol = 330. (IFCLENGTHMEASURE) [MILLI METRE]
    Hauteur de Levage Max = 5850. (IFCLENGTHMEASURE) [MILLI METRE]
    Hauteur hors tout = 1920. (IFCLENGTHMEASURE) [MILLI METRE]
    Largeur hors tout = 1810. (IFCLENGTHMEASURE) [MILLI METRE]
    Longueur hors tout au tablier = 3830. (IFCLENGTHMEASURE) [MILLI METRE]
  Electrical - Loads | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Circuit Number = "" (IFCTEXT)
    Panel = "" (IFCTEXT)
  Phasing | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Phase Created = "New Construction" (IFCLABEL)
  Pset_AirSideSystemInformation | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "Level 1" (IFCLABEL)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Building Story = TRUE (IFCBOOLEAN)
    Name = "Level 1" (IFCTEXT)
    Structural = FALSE (IFCBOOLEAN)
  Identity Data | properties | on 1 type object
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    BC_MODEL_ID = "760538" (IFCTEXT)
    BC_OBJECT_ID = "214593" (IFCTEXT)
    BC_OBJECT_VERSION = "#1" (IFCTEXT)
    BC_VARIANT_ID = "527012" (IFCTEXT)
    Code Name = "" (IFCTEXT)
    Créé par = "ATLANCAD" (IFCTEXT)
    Lien de l'Objet sur le site fabricant = "https://www.manitou.com/" (IFCTEXT)
    Manufacturer = "MANITOU" (IFCTEXT)
    Model = "MT 625" (IFCTEXT)
    Numéro d'article commerce international (NACI) = "" (IFCTEXT)
    OmniClass Number = "23.50.30.00" (IFCTEXT)
    OmniClass Title = "Materials Handling" (IFCTEXT)
    Référence = "MT 625" (IFCTEXT)
    Type Comments = "Télescopique fixe compact" (IFCTEXT)
    Type Name = "MT 625" (IFCTEXT)
    Type de l'Objet = "" (IFCTEXT)
    URL = "www.manitou.com" (IFCTEXT)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    IsLandmarked = UNKNOWN (IFCLOGICAL)
    NumberOfStoreys = 1 (IFCINTEGER)
  Constraints(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation Base = "Project Base Point" (IFCIDENTIFIER)
  Graphics(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Color = 0 (IFCINTEGER)
    Line Pattern = "Solid" (IFCLABEL)
    Line Weight = "1" (IFCIDENTIFIER)
    Symbol at End 1 Default = FALSE (IFCBOOLEAN)
    Symbol at End 2 Default = TRUE (IFCBOOLEAN)
  Identity Data(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Type Name = "Level 1" (IFCTEXT)
  Other(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family Name = "Level" (IFCTEXT)
  Construction | properties | on 1 type object
    Bruit au poste de conduite (LpA) en dB(A) = 76. (IFCREAL)
    Bruit à l'environnement (LwA) en dB(A) = 104. (IFCREAL)
    Capacité Réservoir = 0.063 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Consommation moyenne = 0.00153888888888889 (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Nombre de Roue Motrice = 4. (IFCREAL)
    Poids à vide avec fourches = 4800. (IFCMASSMEASURE) [KILO GRAM]
    Puissance du moteur I.C. (ch) = 75. (IFCREAL)
    Puissance du moteur I.C. (kW) = 55.4 (IFCREAL)
  Data | properties | on 1 type object
    Engine norm = "Stage V" (IFCTEXT)
    External turning radius over tyres = 2300. (IFCLENGTHMEASURE) [MILLI METRE]
    Ground clearance = 330. (IFCLENGTHMEASURE) [MILLI METRE]
    Norme du moteur = "Stage V" (IFCTEXT)
    Overall height = 1920. (IFCLENGTHMEASURE) [MILLI METRE]
    Overall length to carriage = 3830. (IFCLENGTHMEASURE) [MILLI METRE]
    Overall width = 1810. (IFCLENGTHMEASURE) [MILLI METRE]
    Tilt-down angle = 117. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Tilt-up angle = 12. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Unladen weight (with forks) = 4800. (IFCMASSMEASURE) [KILO GRAM]
    Wheelbase = 3310. (IFCLENGTHMEASURE) [MILLI METRE]
  Energy Analysis | properties | on 1 type object
    Average consumption (L/h) = 5.54 (IFCREAL)
    I.C. Engine power rating - Power (ch) = 75. (IFCREAL)
    I.C. Engine power rating - Power (kW) = 55.4 (IFCREAL)
  Green Building Properties | properties | on 1 type object
    Emission de CO2 = 0. (IFCREAL)