IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView_V2.0]"
Description: "ExchangeRequirement []"
Time stamp: "2022-09-12T16:16:23"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "22.0.2.392 - Exporter 22.0.2.392 - Default UI"
Application: "Autodesk Revit 2022 (ENU)" version "2022" identifier "Revit" by Organization "Autodesk Revit 2022 (ENU)"

People and organizations
  Person "dev2NW3Q" of Organization (no name given)
  Owner history of Person "dev2NW3Q" of Organization (no name given) | application "Autodesk Revit 2022 (ENU)" version "2022" identifier "Revit" by Organization "Autodesk Revit 2022 (ENU)" | change NOCHANGE | created 1662992182 (2022-09-12T14:16:22Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  MOMENTOFINERTIAUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"
  LINEARFORCEUNIT: derived
  PLANARFORCEUNIT: derived

Spatial structure
IFCPROJECT
  IFCSITE "Default" | latitude 42° 24′ 53.508911″ | longitude -71° 15′ 29.058837″ | elevation above sea level 0.
    IFCBUILDING | postal address (none given)
      IFCBUILDINGSTOREY "Level 1" | long name "Level 1" | object type "Level:Level 1" | elevation 0.
        contains 1 element
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "FR - MT 930:MT 930" | object type "FR - MT 930:MT 930" | names: "FR - MT 930:MT 930:12202" | material: materials ("<Unnamed>", "255_0_0", "26_26_26", "1_BLANC", "0_0_0", "59_59_59", "255_87_69", "214_217_227", "0_Acier", "1_ROUGE 2") | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Dimensions

Types
  IFCBUILDINGELEMENTPROXYTYPE "FR - MT 930:MT 930" | 1 occurrence | material: materials ("<Unnamed>", "255_0_0", "26_26_26", "1_BLANC", "0_0_0", "59_59_59", "255_87_69", "214_217_227", "0_Acier", "1_ROUGE 2") | property sets: Constraints, Construction, Data, Dimensions, Energy Analysis, Green Building Properties

Property sets
  Pset_ProductRequirements | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY) | on 1 type object
    Category = "Specialty Equipment" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Name = "Level 1" (IFCLABEL)
  Other | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
  Other | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Category = "Specialty Equipment" (IFCLABEL)
    Family = "FR - MT 930: MT 930" (IFCLABEL)
    Family and Type = "FR - MT 930: MT 930" (IFCLABEL)
    Type = "FR - MT 930: MT 930" (IFCLABEL)
    Type Id = "FR - MT 930: MT 930" (IFCLABEL)
  Other | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family = "Level: Level 1" (IFCLABEL)
    Family and Type = "Level: Level 1" (IFCLABEL)
    Type = "Level: Level 1" (IFCLABEL)
    Type Id = "Level: Level 1" (IFCLABEL)
  Other | properties | on 1 type object
    Bruit au poste de conduite (LpA) en dB(A) = 74. (IFCREAL)
    Bruit à l'environnement (LwA) en dB(A) = 103. (IFCREAL)
    Category = "Specialty Equipment" (IFCLABEL)
    Emissions de CO2 (kg/h) = 10.01 (IFCREAL)
    Family Name = "FR - MT 930" (IFCTEXT)
    Load at Max Height = 1500. (IFCMASSMEASURE) [KILO GRAM]
    Load at Max Offset = 450. (IFCMASSMEASURE) [KILO GRAM]
    MasterFormat = "Operation and Maintenance of Transportation" (IFCTEXT)
    Masterformat Code = "34 01 00" (IFCTEXT)
    Maximum Load Supported (Fork or Pod) = 3000. (IFCMASSMEASURE) [KILO GRAM]
    OmniClass code = "23-23 00 00" (IFCTEXT)
    OmniClass description = "Conveying Systems and Material Handling Products" (IFCTEXT)
    Turning Radius = 3.35 (IFCLENGTHMEASURE) [MILLI METRE]
    Uniformat = "Other Conveying Systems" (IFCTEXT)
    Uniformat code = "D1090" (IFCTEXT)
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY) | on 1 type object
    Reference = "MT 930" (IFCIDENTIFIER)
  Pset_ManufacturerTypeInformation | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY) | on 1 type object
    Manufacturer = "MANITOU" (IFCLABEL)
  Pset_QuantityTakeOff | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY) | on 1 type object
    Reference = "MT 930" (IFCIDENTIFIER)
  Constraints | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Elevation from Level = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Host = "None" (IFCTEXT)
    Moves With Nearby Elements = FALSE (IFCBOOLEAN)
    Offset from Host = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 type object
    Capacité max = 3000. (IFCMASSMEASURE) [KILO GRAM]
    Default Elevation = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Déport Max = 6050. (IFCLENGTHMEASURE) [MILLI METRE]
    Hauteur de levage max = 8850. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Abaque Visible = TRUE (IFCBOOLEAN)
    Area = 30.5865429822256 (IFCAREAMEASURE) [SQUARE_METRE]
    Déport max = FALSE (IFCBOOLEAN)
    Déport souhaité = 1254. (IFCLENGTHMEASURE) [MILLI METRE]
    Hauteur de levage souhaitée = -50. (IFCLENGTHMEASURE) [MILLI METRE]
    Rayon de Braquage Visible = TRUE (IFCBOOLEAN)
    Volume = 4.16748089566013 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Computation Height = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 1 type object
    Max Lifting Height = 8850. (IFCLENGTHMEASURE) [MILLI METRE]
    Max Offset = 6050. (IFCLENGTHMEASURE) [MILLI METRE]
    Overall height = 1990. (IFCLENGTHMEASURE) [MILLI METRE]
    Overall width = 1990. (IFCLENGTHMEASURE) [MILLI METRE]
  Electrical - Loads | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Circuit Number = "" (IFCTEXT)
    Panel = "" (IFCTEXT)
  Phasing | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Phase Created = "New Construction" (IFCLABEL)
  Pset_AirSideSystemInformation | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "Level 1" (IFCLABEL)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Building Story = TRUE (IFCBOOLEAN)
    Name = "Level 1" (IFCTEXT)
    Structural = FALSE (IFCBOOLEAN)
  Identity Data | properties | on 1 type object
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    BC_MODEL_ID = "706243" (IFCTEXT)
    BC_OBJECT_ID = "214599" (IFCTEXT)
    BC_OBJECT_VERSION = "#1" (IFCTEXT)
    BC_VARIANT_ID = "527018" (IFCTEXT)
    Code Name = "" (IFCTEXT)
    Créé par = "ATLANCAD" (IFCTEXT)
    GTIN (Global Trade Item Number) = "" (IFCTEXT)
    Manufacturer = "MANITOU" (IFCTEXT)
    Manufacturer Product Link = "https://www.manitou.com/" (IFCTEXT)
    Model = "MT 930" (IFCTEXT)
    Object type = "" (IFCTEXT)
    OmniClass Number = "23.50.30.00" (IFCTEXT)
    OmniClass Title = "Materials Handling" (IFCTEXT)
    Reference = "MT 930" (IFCTEXT)
    Type Comments = "Télescopique fixe compact" (IFCTEXT)
    Type Name = "MT 930" (IFCTEXT)
    URL = "www.manitou.com" (IFCTEXT)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    IsLandmarked = UNKNOWN (IFCLOGICAL)
    NumberOfStoreys = 1 (IFCINTEGER)
  Constraints(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation Base = "Project Base Point" (IFCIDENTIFIER)
  Graphics(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Color = 0 (IFCINTEGER)
    Line Pattern = "Solid" (IFCLABEL)
    Line Weight = "1" (IFCIDENTIFIER)
    Symbol at End 1 Default = FALSE (IFCBOOLEAN)
    Symbol at End 2 Default = TRUE (IFCBOOLEAN)
  Identity Data(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Type Name = "Level 1" (IFCTEXT)
  Other(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family Name = "Level" (IFCTEXT)
  Construction | properties | on 1 type object
    Consommation moyenne = 0.00146666666666667 (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Number of Driving Wheels = 4. (IFCREAL)
    Tank Capacity = 0.09 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Data | properties | on 1 type object
    Angle de cavage = 11. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Angle de déversement = 116. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Empattement = 2690. (IFCLENGTHMEASURE) [MILLI METRE]
    Garde au sol = 350. (IFCLENGTHMEASURE) [MILLI METRE]
    Hauteur hors tout = 1990. (IFCLENGTHMEASURE) [MILLI METRE]
    Largeur hors tout = 1990. (IFCLENGTHMEASURE) [MILLI METRE]
    Longueur hors tout au tablier = 4670. (IFCLENGTHMEASURE) [MILLI METRE]
    Norme du moteur = "Stage V" (IFCTEXT)
    Norme moteur = "Stage V" (IFCTEXT)
    Poids à vide avec fourches = 6550. (IFCMASSMEASURE) [KILO GRAM]
    Rayon de braquage exterieur roues = 3350. (IFCLENGTHMEASURE) [MILLI METRE]
  Energy Analysis | properties | on 1 type object
    Consommation moyenne (L/h) = 5.28 (IFCREAL)
    Puissance du moteur I.C. (ch) = 75. (IFCREAL)
    Puissance du moteur I.C. (kW) = 54.6 (IFCREAL)
  Green Building Properties | properties | on 1 type object
    CO2 = 0. (IFCREAL)