IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView_V2.0]"
Time stamp: "2023-07-04T09:51:47"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "20200210_1400(x64) - Exporter 20.2.12.1 - Interface utilisateur alternative 20.2.12.1"
Application: "Autodesk Revit 2020 (FRA)" version "2020" identifier "Revit" by Organization "Autodesk Revit 2020 (FRA)"

People and organizations
  Person "va.dang" of Organization (no name given)
  Owner history of Person "va.dang" of Organization (no name given) | application "Autodesk Revit 2020 (FRA)" version "2020" identifier "Revit" by Organization "Autodesk Revit 2020 (FRA)" | change NOCHANGE | created 1688457104 (2023-07-04T07:51:44Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"

Spatial structure
IFCPROJECT
  IFCSITE "Default" | latitude 42° 24′ 53.508911″ | longitude -71° 15′ 29.058837″ | elevation above sea level 0.
    IFCBUILDING
      IFCBUILDINGSTOREY "Niveau 1" | long name "Niveau 1" | object type "Niveau:Niveau 1" | elevation 0.
        contains 1 element
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "MRT 2660" | object type "EN MRT 2660:MRT 2660" | names: "EN MRT 2660:MRT 2660:233094" | material: materials ("199_199_199", "59", "26_26_26", "128", "255_255_255", "59_59_59", "Noir cabine", "191_191_191", "Rouge Manitou", "Noir tole", "153_153_153", "Par défaut", "Blanc", "Acier Noir") | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation, Pset_QuantityTakeOff, Autre, Contraintes, Cotes

Types
  IFCBUILDINGELEMENTPROXYTYPE "MRT 2660" | 1 occurrence | material: materials ("199_199_199", "59", "26_26_26", "128", "255_255_255", "59_59_59", "Noir cabine", "191_191_191", "Rouge Manitou", "Noir tole", "153_153_153", "Par défaut", "Blanc", "Acier Noir") | property sets: Analyse d'énergie, Autre, Contraintes, Données, Données d'identification, Pset_BuildingElementProxyCommon

Property sets
  Graphismes(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Couleur = 0 (IFCINTEGER)
    Epaisseur des lignes = "1" (IFCIDENTIFIER)
    Motif des lignes = "Plein" (IFCLABEL)
    Valeur par défaut du symbole à l'extrémité 1 = FALSE (IFCBOOLEAN)
    Valeur par défaut du symbole à l'extrémité 2 = TRUE (IFCBOOLEAN)
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY) | on 1 type object
    Reference = "MRT 2660" (IFCIDENTIFIER)
  Pset_ManufacturerTypeInformation | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY) | on 1 type object
    Manufacturer = "MANITOU" (IFCLABEL)
  Pset_QuantityTakeOff | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY) | on 1 type object
    Reference = "MRT 2660" (IFCIDENTIFIER)
  Autre | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Catégorie = "Informations sur le projet" (IFCLABEL)
  Autre | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Catégorie = "Equipement spécialisé" (IFCLABEL)
    Famille = "EN MRT 2660: MRT 2660" (IFCLABEL)
    Famille et type = "EN MRT 2660: MRT 2660" (IFCLABEL)
    ID du type = "EN MRT 2660: MRT 2660" (IFCLABEL)
    Type = "EN MRT 2660: MRT 2660" (IFCLABEL)
  Autre | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Catégorie = "Niveaux" (IFCLABEL)
    Famille = "Niveau: Niveau 1" (IFCLABEL)
    Famille et type = "Niveau: Niveau 1" (IFCLABEL)
    ID du type = "Niveau: Niveau 1" (IFCLABEL)
    Type = "Niveau: Niveau 1" (IFCLABEL)
  Autre | properties | on 1 type object
    CO2 emissions = 21.85 (IFCREAL)
    Catégorie = "Equipement spécialisé" (IFCLABEL)
    Noise at driving position (LpA) in dB(A) = 0. (IFCREAL)
    Noise to environment (LwA) = 0. (IFCREAL)
    Nom de la famille = "EN MRT 2660" (IFCTEXT)
  Contraintes | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Décalage par rapport à l'hôte = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Hôte = "Niveau : Niveau 1" (IFCTEXT)
    Niveau = "Niveau: Niveau 1" (IFCLABEL)
    Se déplace avec les éléments voisins = FALSE (IFCBOOLEAN)
    Élévation par rapport au niveau = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Contraintes | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elévation = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Contraintes | properties | on 1 type object
    Elévation par défaut = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Max. capacity = 6000. (IFCREAL)
    Max. lifting height = 25900. (IFCLENGTHMEASURE) [MILLI METRE]
    Max. outreach = 21700. (IFCLENGTHMEASURE) [MILLI METRE]
  Cotes | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Actual height = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Actual offset = 5196.37799412495 (IFCLENGTHMEASURE) [MILLI METRE]
    Desired lifting height = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Desired offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    External turning radius (over tyres) = TRUE (IFCBOOLEAN)
    Max offset = FALSE (IFCBOOLEAN)
    Outriggers deployed = FALSE (IFCBOOLEAN)
    Surface = 107.367378650397 (IFCAREAMEASURE) [SQUARE_METRE]
    Turret rotation = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Visible Charts = TRUE (IFCBOOLEAN)
    Volume = 16.2428925570415 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Cotes | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Hauteur de calcul = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Electricité - Charges | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Numéro de circuit = "" (IFCTEXT)
    Panneau = "" (IFCTEXT)
  Phase de construction | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Phase de création = "Nouvelle construction" (IFCLABEL)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Données d'identification | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Etage de bâtiment = TRUE (IFCBOOLEAN)
    Nom = "Niveau 1" (IFCTEXT)
    Structure = FALSE (IFCBOOLEAN)
  Données d'identification | properties | on 1 type object
    Code d'assemblage = "" (IFCTEXT)
    Commentaires du type = "Chariot télescopique rotatif tout terrain" (IFCTEXT)
    Créé par = "ATLANCAD" (IFCTEXT)
    Description de l'assemblage = "" (IFCTEXT)
    Fabricant = "MANITOU" (IFCTEXT)
    Modèle = "MRT 2145" (IFCTEXT)
    Nom de code = "" (IFCTEXT)
    Nom du type = "MRT 2660" (IFCTEXT)
    Numéro OmniClass = "23.50.30.00" (IFCTEXT)
    Titre OmniClass = "Materials Handling" (IFCTEXT)
    URL = "www.manitou.com" (IFCTEXT)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    IsLandmarked = UNKNOWN (IFCLOGICAL)
    NumberOfStoreys = 1 (IFCINTEGER)
  Autre(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Catégorie = "Niveaux" (IFCLABEL)
    Nom de la famille = "Niveau" (IFCTEXT)
  Contraintes(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Base de l'élévation = "Point de base du projet" (IFCIDENTIFIER)
  Données d'identification(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Nom du type = "Niveau 1" (IFCTEXT)
  Analyse d'énergie | properties | on 1 type object
    Average consumption (L/h) = 8.31 (IFCREAL)
    I.C. Engine power rating - Power (ch) = 156. (IFCREAL)
    I.C. Engine power rating - Power (kW) = 115. (IFCREAL)
  Données | properties | on 1 type object
    Engine norm = "Stage V / Tier 4" (IFCTEXT)
    External turning radius over tyres = 4220. (IFCLENGTHMEASURE) [MILLI METRE]
    Ground clearance = 360. (IFCLENGTHMEASURE) [MILLI METRE]
    Overall cab width = 8080. (IFCLENGTHMEASURE) [MILLI METRE]
    Overall height = 3100. (IFCLENGTHMEASURE) [MILLI METRE]
    Overall width = 2500. (IFCLENGTHMEASURE) [MILLI METRE]
    Tilt-down angle = 112. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Tilt-up angle = 12. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Weight = 18000. (IFCREAL)
    Wheelbase = 3050. (IFCLENGTHMEASURE) [MILLI METRE]

Other addresses and roles
  2 x postal address (none given)